##### Таблица 1

|  |  |  |
| --- | --- | --- |
| parameter | IP address or value | № subnet |
| subnet ID подмрежа | **192.168.###.!!!**  | 1 |
| first host address /gateway/ рутер | ***192.168.###.!!!*** |  |
| last host address | 192.168.###.!!! |
| broadcast address | 192.168.###.!!! |
| CIDR notation | /29 |
| subnet mask | 255.255.255.248 |
| number of hosts per subnet | 6 |
| subnet ID подмрежа | **192.168.###.!!!** | 2 |
| first host address /gateway/ рутер | ***192.168.###.!!!*** |  |
| last host address | 192.168.###.!!! |
| broadcast address | 192.168.###.!!! |
| CIDR notation | /29 |
| subnet mask | 255.255.255.248 |
| number of hosts per subnet | 6 |
| subnet ID подмрежа | **192.168.###.!!!** | 3 |
| first host address /gateway/ рутер | ***192.168.###.!!!*** |  |
| last host IP address | 192.168.###.!!! |
| broadcast address | 192.168.###.!!! |
| CIDR notation | /29 |
| subnet mask | 255.255.255.248 |
| number of hosts per subnet | 6 |
| subnet ID подмрежа | **192.168.###.!!!** | 4 |
| first host address /gateway/ рутер | ***192.168.###.!!!*** |  |
| last host address | 192.168.###.!!! |
| broadcast address | 192.168.###.!!! |
| CIDR notation | /29 |
| subnet mask | 255.255.255.248 |
| number of hosts per subnet | 6 |
| subnet ID подмрежа | **192.168.###.!!!** | 5 |
| first host address /gateway/ рутер | ***192.168.###.!!!*** |  |
| last host address | 192.168.###.!!! |
| broadcast address | 192.168.###.!!! |
| CIDR notation | /29 |
| subnet mask | 255.255.255.248 |
| number of hosts per subnet | 6 |
| subnet ID подмрежа | **192.168.###.!!!** | 6 |
| first host address /gateway/ рутер | ***192.168.###.!!!*** |  |
| last host address | 192.168.###.!!! |
| broadcast address | 192.168.###.!!! |
| CIDR notation | /29 |
| subnet mask | 255.255.255.248 |
| number of hosts per subnet | 6 |

##### Таблица 1 /продължение/

|  |  |  |
| --- | --- | --- |
| parameter | IP address or value | № subnet |
| subnet ID подмрежа | **192.168.###.!!!**  | 7 |
| first host address /gateway/ рутер | ***192.168.###.!!!*** |  |
| last host address | 192.168.###.!!! |
| broadcast address | 192.168.###.!!! |
| CIDR notation | /29 |
| subnet mask | 255.255.255.248 |
| number of hosts per subnet | 6 |
| subnet ID подмрежа | **192.168.###.!!!** | 8 |
| first host address /gateway/ рутер | ***192.168.###.!!!*** |  |
| last host address | 192.168.###.!!! |
| broadcast address | 192.168.###.!!! |
| CIDR notation | /29 |
| subnet mask | 255.255.255.248 |
| number of hosts per subnet | 6 |